Four pots – each defines the acceleration for 25% of the bar length

Click button for manual reset

|  |  |
| --- | --- |
| Hold button and turn | Function and LED indication |
| POTA | Bar length   * 4 input steps * 8 input steps * 16 input steps (default) * 32 input steps |
| POTB | Output rate multiplier   * Divide by 2 * 1:1 (default) * Multiply by 2 * Multiply by 4 |
| POTC | Reset mode   * Restart and run freely (default) * Restart and run once * Restart and run only while high * Run while high, do not reset |
| POTD | Internal clock tempo (when no external clock) – 30 .. 220bpm |